**SMART PARKING (PHASE 3)**

**IoT can be used in parking management:**

The rapid demand for parking spaces stems from two major trends – urbanization and car ownership. In a short period, the IoT-based parking management system has positively impacted all stakeholders involved in the process.

For instance, drivers can plan trips and commutes keeping slot occupancy in mind. Enforcement agencies can detect and evaluate the gravity of parking rules violations in seconds.

Parking facility managers can optimize the use of the personnel and the available space. Adding to that thought, IoT can be used in parking management in the following ways:

* Create “smart” parking meters that accept payments via credit card or smartphone and provide real-time information on space availability.
* Extend the operating time of an autonomous parking system by consuming less power with the help of LoRaWAN® networking standard.
* Send real-time data from IoT sensors to a cloud server and share it with users to provide them with the details of free-parking spaces.
* Determine the number and position of vacant parking spaces precisely using [**IoT sensors**](https://www.intuz.com/guide-on-top-iot-sensor-types).
* Reduce congestion and improve traffic flow by using sensors to monitor parking space availability and direct drivers to available spaces.
* [**IoT gateway**](https://www.intuz.com/blog/the-workings-of-an-iot-gateway) and the LPWAN protocol help connect IoT devices and sensors in sizable parking lots.
* The parking management company can use a cloud-based IoT dashboard. It uses gathered sensor data to mine intelligible insights that are visually appealing and provides a clear picture of the parking facility.
* Optimize parking operations and improve security by tracking vehicles entering and exiting a parking facility.
* [**Mobile applications**](https://www.intuz.com/mobile-app-development-guide) can display parking data to drivers and send alerts in case of a security breach.
* Monitor environmental conditions in parking garages, such as air quality and temperature, to ensure the safety of occupants.

**SOURCE CODE:**

import time

import RPi.GPIO as GPIO

import time

import os,sys

from urllib.parse import urlparse

import paho.mqtt.client as paho

GPIO.setmode(GPIO.BOARD)

GPIO.setwarnings(False)

'''

define pin for lcd

'''

# Timing constants

E\_PULSE = 0.0005

E\_DELAY = 0.0005

delay = 1

# Define GPIO to LCD mapping

LCD\_RS = 7

LCD\_E = 11

LCD\_D4 = 12

LCD\_D5 = 13

LCD\_D6 = 15

LCD\_D7 = 16

slot1\_Sensor = 29

slot2\_Sensor = 31

GPIO.setup(LCD\_E, GPIO.OUT) # E

GPIO.setup(LCD\_RS, GPIO.OUT) # RS

GPIO.setup(LCD\_D4, GPIO.OUT) # DB4

GPIO.setup(LCD\_D5, GPIO.OUT) # DB5

GPIO.setup(LCD\_D6, GPIO.OUT) # DB6

GPIO.setup(LCD\_D7, GPIO.OUT) # DB7

GPIO.setup(slot1\_Sensor, GPIO.IN)

GPIO.setup(slot2\_Sensor, GPIO.IN)

# Define some device constants

LCD\_WIDTH = 16 # Maximum characters per line

LCD\_CHR = True

LCD\_CMD = False

LCD\_LINE\_1 = 0x80 # LCD RAM address for the 1st line

LCD\_LINE\_2 = 0xC0 # LCD RAM address for the 2nd line

LCD\_LINE\_3 = 0x90# LCD RAM address for the 3nd line

def on\_connect(self, mosq, obj, rc):

self.subscribe("Fan", 0)

def on\_publish(mosq, obj, mid):

print("mid: " + str(mid))

mqttc = paho.Client() # object declaration

# Assign event callbacks

mqttc.on\_connect = on\_connect

mqttc.on\_publish = on\_publish

url\_str = os.environ.get('CLOUDMQTT\_URL', 'tcp://broker.emqx.io:1883')

url = urlparse(url\_str)

mqttc.connect(url.hostname, url.port)

'''

Function Name :lcd\_init()

Function Description : this function is used to initialized lcd by sending the different commands

'''

def lcd\_init():

# Initialise display

lcd\_byte(0x33,LCD\_CMD) # 110011 Initialise

lcd\_byte(0x32,LCD\_CMD) # 110010 Initialise

lcd\_byte(0x06,LCD\_CMD) # 000110 Cursor move direction

lcd\_byte(0x0C,LCD\_CMD) # 001100 Display On,Cursor Off, Blink Off

lcd\_byte(0x28,LCD\_CMD) # 101000 Data length, number of lines, font size

lcd\_byte(0x01,LCD\_CMD) # 000001 Clear display

time.sleep(E\_DELAY)

'''

Function Name :lcd\_byte(bits ,mode)

Fuction Name :the main purpose of this function to convert the byte data into bit and send to lcd port

'''

def lcd\_byte(bits, mode):

# Send byte to data pins

# bits = data

# mode = True for character

# False for command

GPIO.output(LCD\_RS, mode) # RS

# High bits

GPIO.output(LCD\_D4, False)

GPIO.output(LCD\_D5, False)

GPIO.output(LCD\_D6, False)

GPIO.output(LCD\_D7, False)

if bits&0x10==0x10:

GPIO.output(LCD\_D4, True)

if bits&0x20==0x20:

GPIO.output(LCD\_D5, True)

if bits&0x40==0x40:

GPIO.output(LCD\_D6, True)

if bits&0x80==0x80:

GPIO.output(LCD\_D7, True)

# Toggle 'Enable' pin

lcd\_toggle\_enable()

# Low bits

GPIO.output(LCD\_D4, False)

GPIO.output(LCD\_D5, False)

GPIO.output(LCD\_D6, False)

GPIO.output(LCD\_D7, False)

if bits&0x01==0x01:

GPIO.output(LCD\_D4, True)

if bits&0x02==0x02:

GPIO.output(LCD\_D5, True)

if bits&0x04==0x04:

GPIO.output(LCD\_D6, True)

if bits&0x08==0x08:

GPIO.output(LCD\_D7, True)

# Toggle 'Enable' pin

lcd\_toggle\_enable()

'''

Function Name : lcd\_toggle\_enable()

Function Description:basically this is used to toggle Enable pin

'''

def lcd\_toggle\_enable():

# Toggle enable

time.sleep(E\_DELAY)

GPIO.output(LCD\_E, True)

time.sleep(E\_PULSE)

GPIO.output(LCD\_E, False)

time.sleep(E\_DELAY)

'''

Function Name :lcd\_string(message,line)

Function Description :print the data on lcd

'''

def lcd\_string(message,line):

# Send string to display

message = message.ljust(LCD\_WIDTH," ")

lcd\_byte(line, LCD\_CMD)

for i in range(LCD\_WIDTH):

lcd\_byte(ord(message[i]),LCD\_CHR)

lcd\_init()

lcd\_string("welcome ",LCD\_LINE\_1)

time.sleep(0.5)

lcd\_string("Car Parking ",LCD\_LINE\_1)

lcd\_string("System ",LCD\_LINE\_2)

time.sleep(0.5)

lcd\_byte(0x01,LCD\_CMD) # 000001 Clear display

# Define delay between readings

delay = 5

while 1:

# Print out results

rc = mqttc.loop()

slot1\_status = GPIO.input(slot1\_Sensor)

time.sleep(0.2)

slot2\_status = GPIO.input(slot2\_Sensor)

time.sleep(0.2)

if (slot1\_status == False):

lcd\_string("Slot1 Parked ",LCD\_LINE\_1)

mqttc.publish("slot1","1")

time.sleep(0.2)

else:

lcd\_string("Slot1 Free ",LCD\_LINE\_1)

mqttc.publish("slot1","0")

time.sleep(0.2)

if (slot2\_status == False):

lcd\_string("Slot2 Parked ",LCD\_LINE\_2)

mqttc.publish("slot2","1")

time.sleep(0.2)

else:

lcd\_string("Slot2 Free ",LCD\_LINE\_2)

mqttc.publish("slot2","0")

time.sleep(0.2)

**SENSORS**

**ULTRASONIC SENSOR:**

An ultrasonic sensor is an instrument that measures the distance to an object using ultrasonic sound waves. An ultrasonic sensor uses a transducer to send and receive ultrasonic pulses that relay back information about an object's proximity.It is used to check whether there is vehicle in particular slot or not.

Ultrasonic sensor is installed on the ceiling above a parking space and the distance from the ceiling to the ground is measured using a backward echo wave from the ultrasonic sensor. This distance is used as a basic value to determine the vehicle parking status.

**IR SENSOR:**

**IR sensor is an electronic device, that emits the light in order to sense some object of the surroundings. An IR sensor can measure the heat of an object as well as detects the motion. Usually, in the infrared spectrum, all the objects radiate**

**working principle of an infrared sensor is similar to the object detection sensor. This sensor includes an IR LED & an IR Photodiode, so by combining these two can be formed as a photo-coupler otherwise optocoupler. The physics laws used in this sensor are planks radiation, Stephan Boltzmann & weins displacement.**

**senses the incoming car then the signal is transmitted to the DC motor to open the gate. The display is placed at the entrance to show the available parking space. An IR sensor 1 is placed at the entrance to count the entering cars. Once the IR sensor**

**MAGNETOMETER:**

Magnetic parking sensors should be placed one-third of the way in front of the parking space. The sensor can detect parked vehicles with high accuracy regardless of parking mode and vehicle type

**RADAR:**

Smart Parking Sensor Technolgy is a radar sensor device that allows the detection of parking availability indoors and outdoors. Wireless detection of parking spot occupancy. Best accuracy in the market: radar and magnetic technology combination